**Simplified Test Plan**

Testing will be done primarily on the speed of data transfer between the Rpi3 and the Rpi zero. The tests will be done using 2-3 different types of encryption and with different data sizes and transfer rates. Currently, the plan is to use 25 total outputs for each type of encryption to determine how the efficiency of each is affected under the different circumstances previously listed. Each encryption type will be tested individually, but under the same conditions with no unnecessary processes running in the background. The final results of each test will be stored in an excel table using the transfer time, receive time, and total time as the outputs.